**Release note**

|  |  |
| --- | --- |
| **version** | Openncc CDK R20.12.02 |
| **Release date** | 2020.12.18 |
| **Improvement** | 1.modify firmware usb pid from F63B to F63D  2.resolve losted frame bug in firmware  3.modify sdk update pid to f63d too. |
| **Known issue** | 1: View for windows will collapsed when switch ai mode many times.  2:AR0234 sensor exposed issue.  3:It will been crashed just used ai mode “face-detection-retail-0004-fp16” when used AR0234 sensor. |
| **compatibility** |  |
| **Notes:** |  |